GUERNSEY COUNTY HIGHWAY DEPARTMENT

PERMIT#\_\_\_\_\_\_\_\_

RECEIPT OF FEES

$\_\_\_\_PD on \_\_\_\_\_ Cash or CK#\_\_\_\_\_

***ROAD OPEN CUT PERMIT***

Agreement between the Guernsey County Engineer, Cambridge, Ohio and \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_, for permission to install \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_­­­­\_\_\_\_\_\_\_\_within the public right-of-way limits of (Road #) \_\_\_\_\_\_\_\_\_\_\_\_\_ (Road Name) \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_. Nature of work: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Extent and limits of work: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Number of Crossings\_\_\_\_

The following conditions shall be met, if deemed necessary by the County Engineer, by the above-named Company during construction:

1. The County Engineer’s office shall be notified not less than two working days prior to the start of the work, by calling the Guernsey County Engineer’s office. (740) 432-2234
2. All crossings shall be made at a minimum depth of 30 inches, buried not less than 18 inches below the surface of the berm nor less than 18 inches below the ditch line. Utilities shall extend four (4) feet from the edge of the paved surface of the road and said utility also shall not be placed within ten (10) feet of any part of a culvert, bridge structure, or wing walls.
3. Utilities proposed within the County Road Right of way shall be field located and agreed to by the County Engineer’s Office prior to installation. Detailed plans shall be attached to this Permit application.
4. Should the road surface, culverts, pipes and road structures be damaged as a result of the construction work, they shall be replaced or restored to their original condition without any cost to Guernsey County.
5. No dirt or other waste materials shall be left on site. The road surface and the road R/W will be reclaimed to ideal original condition.
6. Bridge load limits shall be observed and conformed to as specified at given bridges.
7. All safety precautions necessary to protect the traveling public shall be taken. Crossings and underground utilities will be marked by posts with labels at both sides of the road.
8. The County will not be responsible or liable for property damage and said Company shall indemnify and save harmless said County of Guernsey from any and all claims, demands, actions, or causes of action from said damages to persons or property arising from permission herein granted.
9. A non-refundable permit fee of $2000.00 is required for each crossing.
10. All utility companies must be properly notified of any construction by calling OUPS 811 or 1-800-362-2764.
11. Failure to comply with the conditions set forth shall be grounds for permit revocation.
12. Permit must bear signatures of all appropriate officials and be approved by the Guernsey County Engineer before construction.



5-4-19