PERMIT#\_\_\_\_\_\_\_\_

RECEIPT OF FEES

$\_\_\_\_PD on \_\_\_\_\_ Cash or CK# \_\_\_\_\_

GUERNSEY COUNTY HIGHWAY DEPARTMENT

***ROAD RIGHT OF WAY WORK PERMIT***

Agreement between the Guernsey County Engineer, Cambridge, Ohio and**Click or tap here to enter text.**, for permission to install **Click or tap here to enter text.**within the public right-of-way limits of (Road #)**Click or tap here to enter text.** (Road Name) **Click or tap here to enter text.** Nature of work: Click or tap here to enter text.

Extent and limits of work: **Click or tap here to enter text.**

The following conditions shall be met, if deemed necessary by the County Engineer, by the above-named Company during construction:

1. The County Engineer’s office shall be notified not less than two days prior to the start of the work, by calling the Guernsey Engineer’s office. (740) 432-2234
2. Said utility shall be buried not less than 18 inches below the surface of the ground or ditch line.
3. Should the road surface, culverts, pipes and road structures be damaged as a result of the utilities construction work, the above item shall be restored to its original condition by the permittee.
4. Bridge load limits shall be observed and conformed to as specified at given bridges.
5. No dirt or other waste materials shall be left on the road surface or within the right-of-way.
6. All safety precautions necessary to protect the traveling public shall be taken.
7. Further, the County will not be responsible or liable for property damage and said Company shall indemnify and save harmless said County of Guernsey from any and all claims, demands, actions, or causes of action from said damages to persons or property arising from permission herein granted.
8. A non-refundable permit fee of $200.00 is required plus an additional permit for each crossing.
9. All utility companies must be properly notified of any construction by calling 1-800-362-2764.
10. Failure to comply with the conditions set forth shall be grounds for permit revocation.
11. Permit must bear signatures of all appropriate officials and be approved by the Guernsey County Engineer before construction.
12. All utilities shall be installed a minimum of four (4) feet from the edge of the paved surface of the road and said utility also shall not be placed nearer than ten (10) feet from any part of culvert, bridge structure, or wing walls, unless otherwise approved by the Guernsey County Engineer.
13. No installation of underground utilities shall be installed within 10’ laterally and 24” vertically of existing County water, sanitary, or storm sewer infrastructure. Crossings shall be done at or near perpendicular.

 COMPANY NAME, ADDRESS, PHONE, EMAIL Approved by:

 Click or tap here to enter text. GUERNSEY COUNTY ENGINEER

 Click or tap here to enter text. 62782 Bennett Ave

 Click or tap here to enter text. Cambridge, Ohio 43725

 Click or tap here to enter text. p. (740) 432-2234 fax (740) 432-5653

 Click or tap here to enter text.

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_

 Foreman, Guernsey County Highway Dept date

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_

 Signature\* date

 \*By signing, I agree to the terms & conditions listed above

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_

 Guernsey County Engineer date

4/28/21